{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["竞品功能调研"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"竞品功能调研","index":0,"n_rows":87,"n_cols":8,"rows_kept":87,"cut":false,"hidden":false,"merged":[[38,1,38,6],[67,1,67,6],[75,1,75,6],[79,1,79,6],[83,1,83,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[14,1,14,6],[26,1,26,6],[2,2,2,6],[3,2,3,6],[4,2,4,6],[5,2,5,6],[6,2,6,6],[7,2,7,6]]}
[]
[]
[null,1,"为了使界面更加简洁直观易用，是否考虑不适用分级菜单，\n而是直接使用明显的命令按钮直接切换各个主功能区界面，而后在各主功能区内进行子功能导航：\n检测分析：规程设置、执行分析、结果展示\n硬件设置：主窗口内已Tab分页形式分类\n基础设置：主窗口内已Tab分页形式分类\n关于：主窗口内版本、联络信息、授权、系统信息等\n帮助：主窗口区不切换，直接打开外部帮助文档"]
[null,2,"只针对光镜配套检测分析，不支持电镜"]
[null,3,"全部检测分析后，是否需要支持在不重新拍照的情况下，更改标准重新分析"]
[null,4,"需要内置多种常见的规程"]
[null,5,"需要内置多种常见的流程（分类管理）"]
[]
[]
[]
[]
[]
[]
[null,"序号","功能特点","Carl Zeiss AxioVision","Jomesa\nHFD","Leica\nCleanliness","OPTION\nOCAAS"]
[null,"硬件控制"]
["※",{"$f":"ROW()-15","v":1},"支持自动扫描台","√","√","√","√","扫描台用哪个厂商？基于哪些硬件开发（扫描台、相机）"]
[null,{"$f":"ROW()-15","v":2},"支持控制SEM成像和EDS分析（电镜）",null,"√",null,"×","×"]
["※",3,"支持模块控制（控制模块自动切换，如切换偏光明场）","√",null,"√","√","自动、手动需要支持"]
["※",4,"手动切换模块时，软件自动识并进行适配","√",null,null,"√","需要根据哪套机型才可以确定是否支持（scopt 还是v8)"]
[null,5,"整合各显微镜、数码设备、三轴电动扫描台",null,"√","√","√","三轴电动扫描台"]
["※",6,"支持设置相机模式、自动聚焦、曝光时间、拍照等功能",null,null,"√","√"]
[null,7,"支持多种自动聚焦算（补偿聚焦、跟踪聚焦、EFI聚焦）","√","√","√","？"]
["※",8,"设备手动调节焦距时，软件自动同步相关参数",null,null,"√","√","基于硬件相关"]
["※",9,"支持用户设置多个不同区域聚焦",null,null,null,"√"]
["※",10,"软件内置数个标准自动聚焦区域",null,null,null,"√"]
["※",11,"可保存当前设置，如放大倍数，载物台移动步长，曝光时间，相机模式，功能模块，自动聚焦等，测试前一键切换（检查设置）",null,null,"√","√"]
[null,"扫描拍照"]
[null,{"$f":"ROW()-16","v":12},"干涉、双折射图像分析",null,"√",null,"×","×"]
[null,{"$f":"ROW()-16","v":13},"自动明场拍照、偏光拍照，自动分析",null,null,null,"√"]
[null,14,"一次扫描（自动偏光平行拍照、正交拍照，自动分析）",null,null,null,"？"]
[null,15,"支持阴影矫正","√",null,null,"√"]
[null,16,"支持CCD水平对齐校正","√",null,null,"？"]
[null,17,"智能倍率识别模块，标尺实时关联",null,null,null,"？","？基于硬件相关，不确定"]
["※",18,"可以通过实时的预览界面来调整拼图的区域大小","√",null,"√","√"]
[null,19,"扫描过程自动对焦、自动光强、自动拍照，进度实时可见","√","√","√","√"]
["※",20,"自动扫描整个式样（矩形或圆形），自动实时图像拼接","√","√","√","√"]
["※",21,"支持离线图片检测分析（支持离线拼图？）","√",null,null,"？","？"]
[null,22,"支持多滤膜托架的载物台，全部自动拍照分别出报告及组合叠加报告",null,"√"]
[null,"识别分析"]
["※",{"$f":"ROW()-17","v":23},"支持手动添加的标尺",null,null,null,"√"]
["※",{"$f":"ROW()-17","v":24},"自动识别标尺",null,null,null,"√","基于硬件相关"]
[null,25,"内置零部件标准（ISO 16232、VDA 19），是否需要内置油品标准？","√","√","√","√","常见的支持"]
["※",26,"可自定义标准并做相关级别评定","√","√","√","√"]
["※",27,"交互式执行，可以显示或隐藏部分固定的设置",null,null,null,"√"]
["※",28,"可以设置标样单次扫描程序",null,null,null,"？"]
["※",29,"可进行非选定颗粒的计算（Caculate Without）",null,null,null,"√"]
[null,30,"自动颗粒类别识别（金属、非金属、纤维）","√","√","√","√"]
[null,31,"自动统计分析及显示结果与等级","√","√",null,"√"]
[null,32,"使用复杂的边界颗粒拼接算法, 能够对被不同视场分割开的颗粒进行检测、表征和分类",null,null,"√","√"]
[null,33,"可依据不同长宽比的设定对纤维与非纤维进行精确分类",null,null,"√","√"]
[null,34,"样色均值极度不佳的滤膜也能够分析",null,"√",null,"√"]
[null,35,"颗粒编辑提取边界（添加、分割、删除）","√",null,null,"√"]
[null,36,"边界提取（二值化）可与原图进行切换","√",null,null,"√"]
[null,37,"颗粒阈值设定完全依据检测标准（可手动调节）",null,"√",null,"√"]
[null,38,"可注释（文本、标尺）","√",null,null,"√","不需要"]
[null,39,"测量（长度、距离、曲面面积、矩形面积）","√",null,null,"√"]
[null,40,"提供多种统计：颗粒列表、统计结果、直方图",null,null,null,"√"]
[null,41,"结合光镜和电镜的分析，生成化学成分和材料分类报告","√","√",null,"×","×"]
[null,42,"可在交互式预览画面中查看光镜与电镜的综合分析结果，点击可重新定位颗粒，并重新EDX分析","√","√",null,"×","×"]
[null,43,"支持图像序列预览、随时聚焦目标图片颗粒，进行颗粒属性尺寸验证、图像重新定位、重新采集、颗粒重新定位",null,"√","√","√"]
[null,44,"将来自一个过滤过程的多个过滤样品组合到一个单一批次进行分析，并为每个过滤器分配不同的颗粒分类设置",null,null,"√","？"]
[null,45,"与激光诱导击穿光谱 (LIBS)结合，无需将颗粒传输到SEM等设备，即可获得颗粒化学指纹图谱，识别污染源",null,null,"√","×","×"]
["※",46,"自动生成专分析结果（包含清洁度代码、滤膜覆盖率、统计数据、评级、滤片全貌图、最大颗粒照片等信息）","√","√","√","√"]
["※",47,"按照不同的计算方式来进行颗粒数量的换算，如零件数，表面积，体积等",null,null,null,"√"]
["※",48,null,null,"√",null,"√"]
["※",49,"颗粒总数，不同级别颗粒数量，允许颗粒数量，判定展示，分析面积",null,null,null,"√"]
[null,50,"快速（全滤纸扫描分析＜10min），精确（≥5μm），智能（识别金属/非金属/纤维准确率大于90%）",null,null,"√","?","与相关相拼横向比较"]
[null,"报告输出"]
[null,{"$f":"ROW()-18","v":51},"可根据用户自行设定报告模板",null,"√","√","√","所有测量出来的数据都可显示在报表中？水晶报表？"]
[null,{"$f":"ROW()-18","v":52},"支持中英文报告",null,"√",null,"√"]
[null,53,"可保存为PDF报告","√",null,null,"√"]
[null,54,"报告图片能够设置是否显示标尺",null,null,null,"√"]
["※",55,"可以显示颗粒真实颜色，不光是黑白颗粒",null,null,null,"√"]
["※",56,"颗粒高度可选择感兴趣颗粒自动测量（最高点，最低点）",null,null,null,"？","必须z轴电动"]
["※",57,"照片测量数据以及柱形图连接可以自行更改",null,null,null,"√"]
[null,"规程流程"]
["※",{"$f":"ROW()-19","v":58},"轻松地创建、修改、导入、导出、删除及锁定规程",null,null,null,"√"]
[null,{"$f":"ROW()-19","v":59},"所有的测试规程、系统配置、图像数据、分析结果等数据都存储在可溯源的数据库中",null,"√",null,"√"]
["※",60,"自定义工作流、可设定工作流中每步执行是否需要交互",null,null,null,"√"]
[null,"数据管理"]
[null,{"$f":"ROW()-20","v":61},"支持超大图像的拼接、保存与显示",null,"√",null,"？","100X以上，同样与硬件配置相关"]
[null,{"$f":"ROW()-20","v":62},"对已分析项目查看、编辑、删除、导出、变更标准重新分析（部分功能只能管理员操作）",null,null,null,"？"]
[null,63,"安全可靠的数据交互功能（部分功能只能管理员操作）",null,null,null,"√","？"]
[null,"交互操作"]
[null,{"$f":"ROW()-21","v":64},"简单而快捷的操作界面",null,null,null,"√"]
["※",{"$f":"ROW()-21","v":65},"可进行中英文的动态切换",null,null,"√","√"]
["※",66,"个性设定的模块展示、功能菜单及快捷键",null,null,null,"√"]