{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","VDA19-2"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
[]
[null,"No","模块","需求","开发期限","备注"]
[null,{"$f":"ROW()-2","v":1},"聚焦补偿","“手动选择点”的功能追加","2期或以后"]
[null,2,"软件扩展","一些预留功能，如权限、集中处理的接口需要有","2期或以后"]
[null,3,"分析范围","测量区域中的视场应该可以移动，考虑自动检测的通用性。默认中心对齐基础上增加一个可以手动移动视场的功能。","2期或以后","1期预留接口"]
[null,4,"替换图片功能","使用高倍率拍照，替换报告中图片，是否可修改等操作需调研确认","2期或以后"]
[null,5,"VDA19.2标准实现","参照附页[VDA19-2]","2期或以后","该标准不常用，对软件逻辑有影响"]
[null,6,"阈值设定需要交互","性能问题：大图加载；及二值化轮廓提取","2期或以后"]
[null,7,"磁盘清理","实现自动清理","2期或以后"]
[null,8,"检测分析","多工位滤膜分析","2期或以后"]
[null,9,"审计追踪功能","报告中增加电子签名","2期或以后"]
[null,10,"审计追踪功能","修改后可查询用户对规程中进行了设置的详细内容的记录","2期或以后"]
[null,11,"成分分析","结合电镜，进行颗粒的成分分析","2期或以后"]
[null,12,"结果查看","提供拼接后大图查看功能（可放大查看细节），参照av的评估图","2期或以后"]
[null,13,"55%亮度问题","偏光模式下，自动调整曝光时间，使滤膜背景灰度为最大灰度的55%±5","2期或以后"]
[null,14,"规程设置、检测","物相提取增加吸管功能","2期或以后"]
[null,15,"规程设置、检测","关于归一化参数选择需要可设定","2期或以后"]
[null,16,"检测分析（相机扫描）","物相提取交互画面左侧的拼图小图选择，加载小图","2期或以后","考虑界面加载时间目前为不加载小图的，如后期使用过程中必须要加载小图时，再实现此功能。视后期需求。"]

{"sheet":"VDA19-2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}