{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[]}
[]
[null,"序号","一级功能","二级功能","描述"]
["OK",1,"硬件对接","自动显微镜/手动显微镜","可以自动识别标尺，或者可以自动识别手动添加的标尺","无法获取物镜位置，因此不能进行自动标尺识别"]
[null,null,null,"载物台"]
["OK",null,null,"相机","拍照，曝光时间，等基本测量功能需要存在"]
["OK",null,null,"模块控制","软件可以控制模块的自动切换，或者手动切换偏光明场的时候，软件也适配"]
["OK",2,"设置功能","硬件参数设置","可以对当前硬件组合（放大倍数，载物台移动步长，曝光时间，相机模式，功能模块，自动聚焦）进行保存，并在测试开始之前能一键切换到设置好的状态"]
[null,null,null,"可以通过实时的预览界面来调整拼图的区域大小","可以进行多点聚焦，用户可以设置不同区域，或者软件内置几个标准的自动聚焦区域"]
[null,null,null,"拼图区域设置","可以通过实时的预览界面来调整拼图的区域大小"]
[null,null,null,"测量参数设置"]
[null,null,null,"分级设置","添加标准，以及判定，可以另存多个分级选项，并且进行调用，非选定颗粒的计算（caculate without）","添加行业标准"]
[null,null,null,"基础设置"]
[null,null,null,"报告模板设置","照片测量数据以及柱形图连接可以自行更改","涉及第三方插件，最优选择"]
[null,null,null,"测试程序设置","可以导入导出，以及删除，可以新建或者修改，或者锁定"]
[null,null,null,"图像来源设置","可以实时拼图或者离线分析图片"]
[null,3,"分析程序","结果展示","滤膜覆盖率"]
[{"$nulls":4},"颗粒总数，不同级别颗粒数量，允许颗粒数量，判定展示，分析面积"]
[{"$nulls":4},"清洁度代码展示"]
[{"$nulls":4},"按照不同的特征参数可以重新排列颗粒"]
[{"$nulls":4},"报告图片能够设置是否显示标尺"]
[null,null,null,"分析执行程序","交互式执行，可以显示或隐藏部分固定的设置"]
[{"$nulls":4},"可以设置标样单次扫描程序"]
[null,null,null,"报告输出","可以显示颗粒真实颜色，不光是黑白颗粒"]
[null,4,"其他功能","工作流","可以自己编写工作流"]
[null,null,null,"颗粒高度","颗粒高度可以选择感兴趣颗粒测量（最高点，最低点）自动测量最好"]
[null,null,null,"数量换算","按照不同的计算方式来进行颗粒数量的换算（零件数，表面积，体积）"]
[null,null,null,"中英文切换","最好是可以进行中英文的切换","界面外观不美观"]
[null,null,null,"多操作者使用快捷方式","多个快捷方式，每个快捷方式里的参数独立设置"]