	
	JOMESA阅美测量系统 



Cleanliness Analysis according to Ford_ESHL1P-7W092
	Description of sample

	Component:

零件
	{Componentl
	Date of Extraction:

清洗日期
	{ Date of Extraction

	Comp. No.:

零件号
	{Component No.
	Examiner:

检测员
	{ Examiner

	Sample No.:

制样编号
	{Sample No.
	Date of Analysis:

分析日期
	{ Date of Analysis

	Customer:

客户
	{Customer
	Specification:
标准
	D_E14/F_I11/J_K0


	Extraction

	Method: 
方法
	{ Method
	Components on filter:

滤膜上零件数量
	{Components on Filter

	Liquid: 
溶剂
	{ Liquid
	Comp. Surface [cm²]:

零件表面积
	{ Comp. Surface [cm²]]

	Amount [L]:

溶剂量
	{Amount Extraction Liquid
	Filter Type:

滤膜类型
	{Type of Filtermembrane

	Weight [mg] :

重量
	{ Weight [mg ]
	


	Microscopic Analysis

	Scale比例尺:
	{ Scale
	Eval. Diameter分析直径[mm]:
	{ Evaluation Diameter [mm]


	Largest metallic particle最大金属 
	Length长 [µm]:
	Met_1L
	Width宽 [µm]:
	{Met_1W

	Largest nonmetallic particle1最大非金属
	Length长 [µm]:
	{pos_woFL
	Width宽 [µm]:
	{pos_woF_W


	Length of largest fiber2 [µm] :

最长纤维
	{1 Fl
	Total length of fibers2 [mm]:

纤维总长度
	{Sum Fibres]


	
	
	Particle count1
per 1000 cm²每1000 cm²

	Particle size

等级[µm]
	Code
代码
	Particle upper Limit

允许颗粒数量上限
	Total1

总数
	Metallic

金属


	Summarized results汇总:

	         > 600
	J-K
	1
	{AwoF_J-K
	{AMet_J-K

	  100 - 600
	F-I
	2000
	{AwoF_F-I
	{AMet_F-I

	    25 - 100
	D-E
	16000
	{AwoF_25_100
	{AMet_25_100


	Detailed results明细:

	         > 1000
	K
	
	{AwoF_K
	{AMet_K

	  600 - 1000
	J
	
	{AwoF_
	{AMet_J

	  400 -   600
	I
	
	{AwoF_I 
	{AMet_I

	  200 -   400
	H
	
	{AwoF_H
	{AMet_H

	  150 -   200
	G
	
	{AwoF_G
	{AMet_G

	  100 -   150
	F
	
	{AwoF_F
	{AMet_F

	    50 -   100
	E
	
	{AwoF_E
	{AMet_E

	    25 -     50
	D
	
	{AwoF_D
	{AMet_D

	    15 -     25
	C
	
	{AwoF_C
	{AMet_C

	      5 -     15
	B
	
	{AwoF_B
	{AMet_B


1: Particles without fibers不含纤维
2: Definition fiber: Nonmetallic, Compactness < {Fiber Comp.-Crit.% or Length/Width > {Fiber L/W-Crit..
   定义纤维与非金属，以面积比<30%或者长/宽>10
	Result

结果
	{Result of


Remarks备注:

Images图像:

	{Image 1}
	{Image 2}

	Largest metallic particle最大金属颗粒
{Met_1L_Copy µm x {Met_1W_Copy µm
	Second largest metallic particle第二大金属颗粒
{Met_2L µm x {Met_2W µm


	{Image 5
	{Image 6

	Largest nonmetallic particle最大非金属颗粒
{pos_woF_1L µm x {pos_woF_1W µm
	Second largest nonmetallic particle第二大非金属颗粒
{NoM_pos_woF_2L µm x {NoM_pos_woF_2W µm


	
	

	Membrane overview滤膜概况
	Largest fiber最长纤维: L = {Fib_1L_Copy µm


{Image 3





{Image 7








